The demo file is only suitable for the model of M500N-16X128RG2.

Please set the config. as follows:

Color: Double Color
Communication Mode: 232 Mode
Width: 128
Height: 16
MOving-Sign Version:L After V3.18
Number stored: 20

