Configure the Sign

Select menu Comm|Sign Config.

1. General Sign Config

Monochrome

The target sign is monochrome and should not display colors.

Address

Change the sign's address.

Group

Change the sign's group.

Width

Change the sign's width.

Height

Change the sign's height.

2. MCS Config

EDV tradition

Enable/Disable the EDV tradition.

Text A Size

Configurations for MCS protocol. It should be enabled when EDV tradition is disabled. User may select a size for Text A(a default file that don't need create) in drop list box.

Timeout

Set the time for timeout. Unit is second(s) .

3. Display Board Config

Warning

We don't advise user change the display board (control card) settings, it should be done in factory.

Change display board settings

If you want to change the display board settings, please select the check box I want to change display board settings.

EN signal inverted

Enable/Disable EN signal inverted for display board. It must be selected check box I want to change display board settings to enable this function at first.

RGB signal inverted

Enable/Disable RGB signal inverted for display board. It must be selected check box I want to change display board settings to enable this function at first.

4. Others Config for Sign

Show On Startup

Set the sign what to display when the sign power up.
| Show Baudrate: Enabled/Disabled show baudrate on sign when power up. Show Sign Address: Enabled/Disabled show sign address on sign when power up. Show Sign Group: Enabled/Disabled show sign group on sign when power up. Show Sign Size: Enabled/Disabled show sign size on sign when power up.

Brightness

Adjust the sign's brightness.

Disable System Beep

Disable /Enable system beep by select or don't select check box Disable System Beep.

NOTE

Click Default button to set all to default.
Click Cancel button to cancel setting and exit the dialog.
Click OK button to confirm setting and exit the dialog.