NetJet Setup

Select menu Comm|Config NetJet (TCP/IP Box).

Connection

Remote Host | The current host name for the NetJet(TCP/IP-RS232 Adapter).
Remote Port | The current port number for the NetJet(TCP/IP-RS232 Adapter).

Configuration

IP Address | The new IP address for the NetJet(TCP/IP-RS232 Adapter).
Subnet Mask | The new subnet mask for the NetJet(TCP/IP-RS232 Adapter).
Gateway | The new gateway for the NetJet(TCP/IP-RS232 Adapter).
Port | The new port number for the NetJet(TCP/IP-RS232 Adapter).
Baudrate | The new baud rate for the NetJet(TCP/IP-RS232 Adapter).

NOTE

The factory default settings for NetJet(TCP/IP-RS232 Adapter) are: IP address 192.1.1.12, port 5005. So before adding the NetJet(TCP/IP-RS232 Adapter) to your local network, you should always config the NetJet(TCP/IP-RS232 Adapter) first.
When config the NetJet(TCP/IP-RS232 Adapter), it needs set your control PC's IP address in the same network with NetJet(TCP/IP-RS232 Adapter) before configuration.
When config the Baudrate for NetJet(TCP/IP-RS232 Adapter), it must be setting as same as LED Sign's.