Insert Sensors(Temperature, Humidity, Dew Point)

Select menu Insert|Sensors(Temperature, Humidity, Dew Point).

Type of Sensor
Select type of sensor, it includes temperature, humidity and dew point.
If select temperature for sensor, it will show above figure.
Display Unit
If this checkbox is not checked, only the number will be displayed.
Precision

Select precision for temperature, it includes six kinds.

Temperature Unit

Select Celsius, Fahrenheit or Kelvin temperature.
If select humidity for sensor, it will show following figure.
Display Unit
If this checkbox is not checked, only the number will be displayed.
Precision
Select precision for humidity, it includes six kinds.
If select dew point for sensor, it will show following figure.
Display Unit
If this checkbox is not checked, only the number will be displayed.
Precision
Select precision for dew point , it includes six kinds.
Dew point Unit
Select Celsius, Fahrenheit or Kelvin for dew point.
If connect one Temperature Sensor and one Temperature/Humidity Sensor to control card at the same time, user can choose the type of sensor to read the temperature value.
Select 'A Temperature' option to read the temperature value from Temperature Sensor(DS18B20).
Select 'B Temperature' option to read the temperature value from Temperature/Humidity Sensor.
When select 'Temperature' option, the program will read the temperature value from Temperature/Humidity Sensor(default). If there is not the Temperature/Humidity Sensor, the program will read the temperature value from Temperature Sensor(DS18B20).

NOTE | The PC software will always dislay number value ??. Only the sign has installed temperature sensor, humidity sensor, or dew point sensor, it can display the temperature, humidity or dew point correctlly.