Sign Brightness

First, please make sure that the communication between control PC and LED Sign is successful.
Then you need to know your control system (WZPMAIN03-Ea + CST-WZP-RSB-02a or WZPMAIN03-Fb + CST-VS-MB-04g later), if your control system is WZPMAIN03-Ea + CST-WZP-RSB-02a, please configure according as Sign Brightness 1; if your control system is WZPMAIN03-Fb + CST-VS-MB-04 or later, please configure according as Sign Brightness 2. Note: If you don't know your control system, you can execute menu Comm|Sign Brightness command, if it can read the current Sign's brightness information, it is WZPMAIN03-Fb + CST-VS-MB-04 or later control system, if it can not read the brightness information, it is WZPMAIN03-Ea + CST-WZP-RSB-02a control system.
Sign Brightness 1
Select menu Comm|Sign Brightness, click [Cancel] button to enter Sign Brightness interface.
User can select brightness adjust mode for Sign.

1. Manual adjustment

Select Manual adjustment from Brightness adjust mode drop list box, and select one brightness value from Brightness value drop list box. Please refer to following figure.
Click OK button to send the brightness value to Sign, the Sign's current brightness will be this value.

2. Auto adjustment

Select Auto adjustment from Brightness adjust mode drop list box.
Click OK button to send auto adjustment brightness command to Sign, the Sign's brightness will be adjusted automatically by light sensor. For this mode, user needs to connect one light sensor to Sign.

3. Schedule adjustment
Select Schedule adjustment from Brightness adjust mode drop list box.

Select time check box, input start time and end time, select brightness value from drop list box, click OK button to send the settings to Sign, the Sign's brightness will be the set value at the set time. Fox example, start time is 8:00, end time is 18:00, select brightness value 60%, then the Sign's brightness is 60% from 8:00 to 18:00 at everyday.
User can set four schedules at most.
Sign Brightness 2
Select menu Comm|Sign Brightness to read current Sign's brightness information, then enter Sign Brightness interface.
User can select brightness adjust mode for Sign.
1. Manual adjustment
Select Manual adjustment from Brightness adjust mode drop list box, and select one brightness value by the slider. Please refer to following figure.
Click OK button to send the brightness value to Sign, the Sign's current brightness will be this value. Note: You can't power off the Sign within one minute after configuring the brightness, otherwise, the brightness settings may be not saved, the Sign may be black or display abnormally.
2. Auto adjustment
Select Auto adjustment from Brightness adjust mode drop list box.
Set Min brightness value and Max brightness value by the sliders, then click OK button to send auto adjustment brightness command to Sign, the Sign's brightness will be adjusted automatically in the set brightness value range by light sensor. For this mode, user needs to connect one light sensor to Sign. Note: You can't power off the Sign within one minute after configuring the brightness, otherwise, the brightness settings may be not saved, the Sign may be black or display abnormally.
3. Schedule Auto adjustment
Select Schedule Auto adjustment from Brightness adjust mode drop list box.
You can set two time segments, and set the minimum brightness value and the maximum brightness value for the two time segments respectively, and the Sign's brightness will be adjusted automatically by light sensor in the time segment and the brightness range.