WZP Overview

WZP is a powerful LED display product based on a real-time multi-tasks operating system, it can display plenty of texts, graphics and animations, and breach restriction of display size(32x240) for E2000 series, for without gray, maximum pixels can reach 256(H)x2048(W), in other words, the maximum height can't exceed 256pixels, and maximum weight can't exceed 2048pixels; for with gray, maximum pixels can reach 256(H)x512(W), in other words, the maximum height can't exceed 256pixels, and maximum weight can't exceed 512pixels. It can actualize multi-line(5lines, 6lines) really; from WZP V1.70 beginning, it can support RGB tricolour without gray display. It is mainly used in some cases where need to display in large size. WZP Sign software is a wonderful software that makes user easily create messages on PC before sending them to the sign. MCS is a full printable character set, easy-learn, full function protocol, which is very popular for user programming LED display controlling.
User can also choose WZP sign for little LED display as small as 8x32 to obtain the outstanding features of this product.
This software is designed for Windows(R) 9x/NT/2000/XP/Win 7.

Key features:

1. | Maximum resolution for without gray: 256(H)¡Á2048(W) pixels, maximum height is 256pixels, maximum weight is 2048pixels, such as, 256(H)x2048(W), 128(H)x1024(W), 128(H)x512(W), 256(H)x256(W), 32(H)x512(W).
2. | Maximum resolution for with gray: 256(H)¡Á512(W), maximum height is 256pixels, maximum weight is 512pixels, such as, 256(H)x512(W), 256(H)x256(W), 128(H)x256(W), 128(H) x 128(W),32(H)x512(W).
3. | Display color : Support single-color, bi-color, tri-color, single-color with gray (8, 256 grade), bi-color with gray (64, 65536 grade), tri-color with gray (256, 65536 grade).
4. | 16MB memory size, FLASH file system data isn't lost easily, it can be saved ten years.
5. | Support many graphics that their format is bmp, gif, png, jpeg and gif animation.
6. | Picture making function, the operation is similar to the draw tool for windows system.
7. | Simple and easy-use gif animation making function.
8. | There are large text edit functions.
| a. Support all fonts in windows(R) system, support all Unicode symbols, it can input all Europe characters. b. Add font outline for text. c. Adjust alignment mode for text. d. Adjust extra spacing between characters and lines. e. Adjust the left, right, top and below position for display content. f. Support tabs of left alignment, and adjust spacing for tabs. g. Support copy and paste for letters, and provide infinite cancelling and repeating function. h. Embed display bmp, gif, png graphics, not support embed gif animation. i. Embed time, temperature, count up and count down.
9. | Support for general counter which can count from an origin value, relative to a given date time, increase or decrease by a given step size, at a given interval.
10. | Time and date format: user defined.
11. | Support daylight saving time display.
12. | Can display temperature, humidity, dew point and speed. The temperature and dew point unit is: Celsius, Fahrenheit or Kelvin, and the humidity unit is: %.
13. | Support manual brightness, auto brightness, or schedule brightness (daylight brightness).
14. | Script provides plenty of display control.
| a. 17 display methods , "rotate" option is used for moving a mass of message leftwards continuously. b. Message speed: 8 message speeds from slowest speed 1 to fastest speed 8. c. Pause time: 0~30 minutes or stop permanently. d. Create many kinds of tasks (such as text, graphic, animation etc.) to run independently, and multi-task can move smoothly at the same time. e. Many subtasks can run according order in sequence task, and set priority for each subtask. f. 7 schedule modes, allow each task to run according appointed time; the subtasks run according their setting time and setting time of father-class sequence task. g. Get corresponding display effect through clicking different nodes.
15. | Communication method: RS232, RS422/485, TCP/IP ( LAN) £¬ Modem £¬ GSM Modem £¬ GPRS MODEM and 3G Modem.
16. | Support for Full-Duplex mode to improve communication speed while using GSM modem or GPRS modem. Please select "Half-Duplex" mode when using RS485 communication mode.
17. | Many signs can be connected in a network.
18. | Support address book function, you can Send the same messages to many signs with different communication modes.
19. | Software remote control on/off display function.
20. | System adjusts time function.
21. | System upgrade: easily upgrade through RS232, RS422 interface.
22. | Prompt online help system; press F1 key on menu, editing box and other positions to get prompt corresponding help information.
23. | The software supports multi-language, it needs stated technology strength, and user needs to translate our appointed file content into the local language, then send them to us and we will translate and edit them.
24. | Plain text MCS protocol provides easy-learn programming control.
| a. Programming control display position, include blurry position and exact position, alignment mode. b. Programming control display method, font, color, speed, pause time etc. c. Customize and install font for MCS protocol. d. Support wide, flicker and other character property controls, support moving and flickering function. e. Support tabs control for many kinds of alignment methods, and adjust spacing for tabs. f. Support embedding some graphics that their format is bmp, gif, png; support embedding gif animation. g. Support embedding time, temperature, count up and count down. h. Support embedding beep. i. Provide 10 stopwatch variables and used for time and pause for sport information. j. Can control the output level for special output port.