Install OS&Font on the Sign

Easily System Upgrate

You can update the OS and fonts on the sign easily through RS232 or RS422 interface.
If the sign's system is damaged by accident, only use COM connection to reinstall the OS on the sign.

Select menu Comm|Install OS&Fonts.

I want to format the target file system

Check this if you want to delete all messages on the sign.

I want to update OS on the sign

Check this if you want to update OS on the sign.
When select this check box, the OS file text should be enabled.
Note: When select the OS file from disk by click Browse button, then click Ok button, it should appear a prompt dialog to power on reset the target, please power on restart the sign.

OS file

Selected the OS file. A default OS file is provide in the software folder.
Click Browse button to select and open OS file from disk.

I want to update fonts on the sign

Check this if you want to update fonts on the sign.
When selected this check box, the Font list box should be enabled.

Add button

Click Add button to add a font type. A default fonts folder is provide in the software folder. User may select and open a font type from Fonts folder.

Remove button

Click Remove button to remove selected font types from Fonts list box.

Up button

Click Up button to move up the selected font types in Fonts list box.

Down button

Click Down button to move down the selected font types in Fonts list box.

Apply button

Click Apply button to add fonts.

OK button

Click OK button to confirm your operation.

Cancel button

Click Cancel button to cancel your operation and exit the dialog.